CBCT and OPG

Advice from Cheema, dental imaging company: Morita X800 – perhaps best for endo

Check dimensions – do we have space of rit

Need to liase with

1. Radiation Protection Advisor (RPA)
2. Our IT
3. Lead lining company
4. Electrician

Cost circa 65K + VAT

4K installation

Training included

May need to buy lap top place Morita software

i-dexel software can be used to send to patients / referring GDP’s.